<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<packages>
<package name="1/4&quot;-STEREO-JACK-SWITCHED">
<description>1/4" TRS jack, with normally-closed switched contacts (closed when unplugged)</description>
</package>
</packages>
<symbols>
<symbol name="1/4&quot;-STEREO-JACK-SWITCHED">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="1/4&quot;-STEREO-JACK-SWITCHED">
<gates>
<gate name="G$1" symbol="1/4&quot;-STEREO-JACK-SWITCHED"/>
</gates>
<devices>
<device name="" package="1/4&quot;-STEREO-JACK-SWITCHED">
<connects>
<connect gate="G$1" pin="P$1" pad="T"/>
<connect gate="G$1" pin="P$2" pad="T-NC"/>
<connect gate="G$1" pin="P$3" pad="R-NC"/>
<connect gate="G$1" pin="P$4" pad="R"/>
<connect gate="G$1" pin="P$5" pad="S-NC"/>
<connect gate="G$1" pin="P$6" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
